1. Please go to this website:
   * <https://elektroautomatik.com/en/>
2. At the top of the website, click on **Software**, then select **Software and Driver**

Graphical user interface, text, application, chat or text message

Description automatically generated

1. Under **More Software from the Categories**, select **Firmwares**

A picture containing graphical user interface

Description automatically generated

1. Scroll down to **your device series** and click on **Download or Link**
2. If taken to the device page, select the **Software** tab and select **Download Firmware updates.zip**

A screenshot of a computer program

Description automatically generated

1. Open the Zip file and extract the files to a new folder on your PC.
2. Download the EA Power Control Software if not already installed on your PC by selecting **Software**, and then **EA Power Control**

Graphical user interface, text, application, chat or text message

Description automatically generated

1. Under **Download & Links**, select **Software**.

Chart

Description automatically generated

1. Using an A to B USB cable, connect the PC to the USB connector on the back of the device.
2. With the device powered on, open the EA Power Control Software.
3. If your device is not shown on the software, click on **Search for Devices**
4. Move the icon for your device to **Update**

Graphical user interface, application

Description automatically generated

1. Select **Browse**

Table

Description automatically generated

1. Open the downloaded firmware update file

Graphical user interface, application

Description automatically generated

1. The Firmware update table will show the current firmware version and the downloaded updated version.

Table

Description automatically generated

The lights will indicate if the update is:

* permissible (green)
* not required (white)
* refused (red)
* permissible, but not recommend, i. e. downgrade (yellow)

Normally, you should only install updates on components with green light

1. Check the component that is to be updated in the column “Install” and then select “Update” at the bottom of the screen.
2. Follow the prompts given as the updates are installed on the device.
3. If updating the HMI firmware, you will be prompted to insert a USB drive into your PC. The firmware will be saved to the USB drive and then can be inserted into the port on the front panel of the device.